IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "bim.house catalog product — reference values, verify with manufacturer"
File name: "ENABLER-BIRUWA-BUGPOLE-KIT-V1.ifc"
Time stamp: "2026-01-01T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 — bim.house product catalog"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE catalog export" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE catalog export" version "1.0" identifier "bim.house" | change ADDED | created 1767225600 (2026-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "美留和 集虫＋間接照明ポール キット v1（CNC/3DPフラットパック・ソーラー自給） (device.house / Enabler)" | long name "BIM.HOUSE" | phase "Catalog product reference model"
  IFCSITE "Catalog Context" | elevation above sea level 0.
    IFCBUILDING "Catalog Building" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Level" | elevation 0.
        contains 1 element
          1 x IFCSANITARYTERMINAL | names: "美留和 集虫＋間接照明ポール キット v1（CNC/3DPフラットパック・ソーラー自給）" | descriptions: "デジタルファブで作って“組み立てるだけ”のキット。CNCルーターで切る焼杉/フェノール合板パネル（タブ＆スロット接合・治具不要）＋3Dプリント（ASA/PETG・屋外UV耐性）の金物・漏斗・クランプ。頂部に集虫ランプ＋漏斗Ø350→捕集ボトルØ200、昼は黒球Ø250（温泉熱加温）＋ネットでアブも捕る。ソーラー100W＋LiFePO4 30Ahで自給、IP66制御箱。間接照明の居場所から虫を林際の一点へ誘導するlure-away設計。弟子屈・美留和ビレッジ用。図面=DXF(R12)＋STL配布。" | property sets: Pset_bimhouse_Catalog

Property sets
  Pset_bimhouse_Catalog | properties | on 1 object (1 IFCSANITARYTERMINAL)
    ListPrice_JPY_excl_tax = 70000 (IFCINTEGER)
    Manufacturer = "device.house / Enabler" (IFCLABEL)
    ModelLabel = "BVK-1" (IFCLABEL)
    Reference = "ENABLER-BIRUWA-BUGPOLE-KIT-V1" (IFCLABEL)
    WarrantyYears = 5 (IFCINTEGER)
    spec_abu = "heated black ball d250 (onsen warm-water coil) + net" (IFCLABEL)
    spec_cnc_parts = "~24" (IFCLABEL)
    spec_collector = "moth-lure lamp + funnel d350 -> jar d200" (IFCLABEL)
    spec_fabrication = "CNC router (12mm phenolic/yakisugi plywood) + FDM 3D print (ASA/PETG)" (IFCLABEL)
    spec_files = "DXF R12 (CNC) + STL (print)" (IFCLABEL)
    spec_ip = "IP66 control box, conformal-coated PCB" (IFCLABEL)
    spec_joinery = "tab-and-slot + minimal bolts" (IFCLABEL)
    spec_materials = "yakisugi/phenolic ply, ASA, stainless fasteners" (IFCLABEL)
    spec_placement = "forest edge, downwind, away from seating (lure-away)" (IFCLABEL)
    spec_power = "solar 100W + LiFePO4 12V 30Ah + MPPT" (IFCLABEL)
    spec_printed_parts = "~12 (brackets/funnel/clamps/grommets)" (IFCLABEL)