IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "bim.house catalog product — reference values, verify with manufacturer"
File name: "ENABLER-BIRUWA-LIGHTBENCH-KIT-V1.ifc"
Time stamp: "2026-01-01T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 — bim.house product catalog"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE catalog export" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE catalog export" version "1.0" identifier "bim.house" | change ADDED | created 1767225600 (2026-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "美留和 間接照明ベンチ キット v1（CNCほぞ組み・温水放射任意） (device.house / Enabler)" | long name "BIM.HOUSE" | phase "Catalog product reference model"
  IFCSITE "Catalog Context" | elevation above sea level 0.
    IFCBUILDING "Catalog Building" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Level" | elevation 0.
        contains 1 element
          1 x IFCFURNISHINGELEMENT | names: "美留和 間接照明ベンチ キット v1（CNCほぞ組み・温水放射任意）" | descriptions: "CNC合板のほぞ組みベンチ。前リップ裏にLEDを内蔵（2200–2700K）し、光源を見せない間接グレージング（低UVで虫を寄せにくい）。座面内にPEX温水管（温泉熱・任意）で放射加温＝温ベンチ。3DプリントのLEDクリップ/配管クランプ。番号付きパーツをスロットで“組み立てるだけ”。弟子屈・美留和ビレッジ用。図面=DXF(R12)。" | property sets: Pset_bimhouse_Catalog

Property sets
  Pset_bimhouse_Catalog | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    ListPrice_JPY_excl_tax = 45000 (IFCINTEGER)
    Manufacturer = "device.house / Enabler" (IFCLABEL)
    ModelLabel = "BVK-2" (IFCLABEL)
    Reference = "ENABLER-BIRUWA-LIGHTBENCH-KIT-V1" (IFCLABEL)
    WarrantyYears = 5 (IFCINTEGER)
    spec_fabrication = "CNC router (plywood)" (IFCLABEL)
    spec_files = "DXF R12" (IFCLABEL)
    spec_heating = "PEX warm loop in seat (onsen, optional, via heat exchanger)" (IFCLABEL)
    spec_joinery = "tab-and-slot" (IFCLABEL)
    spec_lighting = "concealed LED 2200-2700K (no direct glare)" (IFCLABEL)
    spec_printed_parts = "LED clips, pipe clamps" (IFCLABEL)
    spec_seat_h_mm = "420" (IFCLABEL)